[DEVICE]
Name=P16F887
Clock=20000000
[MEMORY_MODEL]
Value=0
[BUILD_TYPE]
Value=0
[ACTIVE_TAB]
Value=uart.c
[USE_EEPROM]
Value=0
[USE_HEAP]
Value=0
[HEAP_SIZE]
Value=0
[EEPROM_DEFINITION]
Value=
[FILES]
Count=1
[BINARIES]
Count=0
[IMAGES]
Count=0
ActiveImageIndex=-1
[OPENED_FILES]
Count=2
File1=uart.c
[EEPROM]
Count=0
[ACTIVE_COMMENTS_FILES]
Count=0
[OTHER_FILES]
Count=0
[SEARCH_PATH]
Count=3
Path0=C:\Users\Public\Documents\Mikroelektronika\mikroC PRO for PIC\Defs\
Path1=C:\Users\Public\Documents\Mikroelektronika\mikroC PRO for PIC\Uses\P16\
Path2=C:\Users\thanhlolthuong\3D Objects\1_HOC TAP\2017 2018 HK2\Do_luong_DKMT\THUCHANH\A_test\code887\
[HEADER_PATH]
Count=0
[HEADERS]
Count=0
[PLDS]
Count=0
[Useses]
Count=5
File0=Button
File1=UART
File2=Sprinti
File3=C_Type
File4=C_String
[EXPANDED_NODES]
Count=0
