#include <nhietdo.h>
#include <lcd4bit.c>
#fuses HS
#fuses nowdt,noprotect,nolvp,xt,put
#use rs232(baud = 9600, parity = n, xmit = pin_c6, rcv = pin_c7, bits = 8)
long adc;
unsigned int8 nhietdo;
void main()
{

   while(TRUE)
   {
      //TODO: User Code
   }

}
