004-005 @READ_PROGRAM_MEMORY8.P1
004-005 @WRITE_PROGRAM_MEMORY8.P2
015     CCP_1_LOW
015     CCP_1
016     CCP_1_HIGH
01B     CCP_2
01B     CCP_2_LOW
01C     CCP_2_HIGH
020     @INTERRUPT_AREA
021     @INTERRUPT_AREA
022     @INTERRUPT_AREA
023     @INTERRUPT_AREA
024     @INTERRUPT_AREA
025     @INTERRUPT_AREA
026     @INTERRUPT_AREA
027     e
028-029 adc
02A     dat
02B     nhietdo
02C-02F @MULFF.P1
02C-02F @SFTOI.P2
02C     LCD_PutChar.cX
02C     LCD_SetData.cX
02C-02D @ITOF.P1
02C     LCD_PutCmd.cX
02C     LCD_SetPosition.cX
030-033 @MULFF.P1
034     @MULFF.@SCRATCH1
035     @MULFF.@SCRATCH2
036     @MULFF.@SCRATCH3
037     @MULFF.@SCRATCH4
038     @MULFF.@SCRATCH5
077     @SCRATCH
078     @SCRATCH
078     _RETURN_
079     @SCRATCH
07A     @SCRATCH
07F     @INTERRUPT_AREA
0FF     @INTERRUPT_AREA
107.6   C1OUT
108.6   C2OUT
10D-10E @READ_PROGRAM_MEMORY8.P1
10D-10E @WRITE_PROGRAM_MEMORY8.P2
17F     @INTERRUPT_AREA
1FF     @INTERRUPT_AREA
27F     @INTERRUPT_AREA
2FF     @INTERRUPT_AREA
37F     @INTERRUPT_AREA
3FF     @INTERRUPT_AREA
47F     @INTERRUPT_AREA
4FF     @INTERRUPT_AREA
57F     @INTERRUPT_AREA
5FF     @INTERRUPT_AREA
67F     @INTERRUPT_AREA
6FF     @INTERRUPT_AREA
77F     @INTERRUPT_AREA
7FF     @INTERRUPT_AREA
87F     @INTERRUPT_AREA
8FF     @INTERRUPT_AREA
97F     @INTERRUPT_AREA
9FF     @INTERRUPT_AREA
A7F     @INTERRUPT_AREA
AFF     @INTERRUPT_AREA
B7F     @INTERRUPT_AREA
BFF     @INTERRUPT_AREA
C7F     @INTERRUPT_AREA
CFF     @INTERRUPT_AREA
D7F     @INTERRUPT_AREA
DFF     @INTERRUPT_AREA
E7F     @INTERRUPT_AREA
EFF     @INTERRUPT_AREA
F7F     @INTERRUPT_AREA
FFF     @INTERRUPT_AREA

ROM Allocation:
000031  rda_isr
000039  @ITOF
000058  @MULFF
0000CF  @SFTOI
0000F0  MAIN
0000F0  @cinit1
00010F  @cinit2

Project Directory:
    C:\Users\thanhlolthuong\3D Objects\1_HOC TAP\2017 2018 HK2\Do_luong_DKMT\THUCHANH\TUAN10\TN4\ccs\

Project Files:
    nhietdo.c                                               [17-Apr-18 08:47  CRC=56E82D66]
    nhietdo.h                                               [17-Apr-18 08:19  CRC=64D0046D]
    ..\..\..\..\..\..\..\..\..\..\Program Files (x86)\PICC\Devices\16F887.h [03-Feb-18 16:29  CRC=6CB1A611]
    ..\..\..\..\..\..\..\..\..\..\Program Files (x86)\PICC\Devices\lcd4bit.c [10-Apr-18 08:42  CRC=ED16C899]
    ..\..\..\..\..\..\..\..\..\..\Program Files (x86)\PICC\Drivers\stddef.h [16-Jul-10 09:27  CRC=897CEC6C]

Source signature=287A7955

Units:
    nhietdo (main)

Compiler Settings:
    Processor:      PIC16F887
    Pointer Size:   16
    ADC Range:      0-1023
    Opt Level:      9
    Short,Int,Long: UNSIGNED: 1,8,16
    Float,Double:   32,32

Output Files:
    XREF file:   nhietdo.xsym
    Errors:      nhietdo.err
    Ext Symbols: nhietdo.esym
    INHX8:       nhietdo.hex
    Symbols:     nhietdo.sym
    List:        nhietdo.lst
    Debug/COFF:  nhietdo.cof
    Project:     nhietdo.ccspjt
    Call Tree:   nhietdo.tre
    Statistics:  nhietdo.STA
